Power on GSE-1

GoPro starts recording video

Save data internally

Write and save data

Main sensors turn on

Telemeter data

Power on TSE-1

Linear Actuator opens

Linear Actuator closes

Motor retracts boom

Motor extends boom

Secondary MCU turns on

End Effector sensors begin transmitting

Power on TSE-2

Start Main MCU